**V**rindavan Technologies

 E-mail : info@vrindavantechnologies.com

 Tel:+91-80-41266977,080-41201590

 

 Ac Adapter

 Input AC: 20 to 250V

 Output: 6V DC Regulated

 Current: 500mA

 Epoxy Molded

 Working Humidity: <95% RH

 Low Ripple Noise

 Inline EMI/RFI Filter

 We can Supply with different connectors